{"text_format":"3","workbook":"xls","n_sheets":7,"sheets":["Table 1","Table 2","Table 3","Table 4","Table 5","Table 6a","Table 6b"],"not_rendered":{"macros":1,"external_links":1,"defined_names":11},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Table 1","index":0,"n_rows":84,"n_cols":7,"rows_kept":84,"merged":[[9,0,61,0],[9,1,14,1],[9,2,14,2],[9,3,14,3],[15,1,34,1],[15,2,20,2],[15,3,20,3],[21,2,27,2],[21,3,27,3],[28,2,34,2],[28,3,34,3],[35,1,41,1],[35,2,41,2],[35,3,41,3],[42,1,47,1],[42,2,47,2],[42,3,47,3],[48,1,54,1],[48,2,54,2],[48,3,54,3],[55,1,61,1],[55,2,61,2],[55,3,61,3],[62,0,83,0],[62,1,67,1],[62,2,67,2],[62,3,67,3],[62,5,67,5],[62,6,67,6],[68,1,74,1],[68,2,74,2],[68,3,74,3],[68,5,74,5],[68,6,74,6],[75,1,81,1],[75,2,81,2],[75,3,81,3],[75,5,81,5],[75,6,81,6],[82,1,83,1],[82,2,83,2]],"flags":["formulas_cached_only"]}
[]
["Northern Gas Networks Limited"]
["Gas Meter Services Contract"]
["Meterwork Contract Rates"]
[]
["Table 1"," "]
["Emergency Services (meter install)"," "]
[{"$nulls":5}," "]
["Activity Job Code","Notes","NGM Job Ref Type","Description",null,"Unit price","Effective Date"]
["EMS02 Meter Install/Fix","Abortive calls/No accesses are included in these rates and cannot be charged separately",2200000000,"LP Diaphragm Meters","U16",{"v":48.52,"d":"£48.52"},"2006-06-01"]
[{"$nulls":4},"U25",{"v":48.52,"d":"£48.52"},"2006-06-01"]
[{"$nulls":4},"U40",{"v":95.8,"d":"£95.80"},"2006-06-01"]
[{"$nulls":4},"U65",{"v":95.8,"d":"£95.80"},"2006-06-01"]
[{"$nulls":4},"U100",{"v":142.92,"d":"£142.92"},"2006-06-01"]
[{"$nulls":4},"U160",{"v":142.92,"d":"£142.92"},"2006-06-01"]
[null,"Genuine abortive visits and third party cancellation charges can be recovered separately and are NOT to be  included in these rates.",2400000000,"MP Diaphragm Meters","U16",{"v":303.86,"d":"£303.86"},"Signature date"]
[{"$nulls":4},"U25",{"v":303.86,"d":"£303.86"},"Signature date"]
[{"$nulls":4},"U40",{"v":340.88,"d":"£340.88"},"Signature date"]
[{"$nulls":4},"U65",{"v":588.24,"d":"£588.24"},"Signature date"]
[{"$nulls":4},"U100",{"v":637.6,"d":"£637.60"},"Signature date"]
[{"$nulls":4},"U160",{"v":691.97,"d":"£691.97"},"Signature date"]
[null,null,2400000000,"LP Rotary/Turbine Meters","RO/TU 50mm/2\"",{"v":372.03,"d":"£372.03"},"Signature date"]
[{"$nulls":4},"RO/TU 80mm/3\"",{"v":490.96,"d":"£490.96"},"Signature date"]
[{"$nulls":4},"RO/TU 100mm/4\"",{"v":663.75,"d":"£663.75"},"Signature date"]
[{"$nulls":4},"RO/TU 150mm/6\"",{"v":795.4,"d":"£795.40"},"Signature date"]
[{"$nulls":4},"RO/TU 200mm/8\"",{"v":992.87,"d":"£992.87"},"Signature date"]
[{"$nulls":4},"RO/TU 250mm/10\"",{"v":992.87,"d":"£992.87"},"Signature date"]
[{"$nulls":4},"RO/TU >250mm 10\"","Quoted","Signature date"]
[null,null,2400000000,"MP Rotary/Turbine Meters","RO/TU 50mm/2\"",{"v":807.14,"d":"£807.14"},"Signature date"]
[{"$nulls":4},"RO/TU 80mm/3\"",{"v":905.88,"d":"£905.88"},"Signature date"]
[{"$nulls":4},"RO/TU 100mm/4\"",{"v":1148.23,"d":"£1,148.23"},"Signature date"]
[{"$nulls":4},"RO/TU 150mm/6\"",{"v":1271.66,"d":"£1,271.66"},"Signature date"]
[{"$nulls":4},"RO/TU 200mm/8\"",{"v":1543.18,"d":"£1,543.18"},"Signature date"]
[{"$nulls":4},"RO/TU 250mm/10\"",{"v":1543.18,"d":"£1,543.18"},"Signature date"]
[{"$nulls":4},"RO/TU > 250mm/10\"","Quoted","Signature date"]
[null,"Charge for fabricating a spool piece for each rig size",null,"Rotary/Turbine Meters","RO/TU 50mm/2\"",{"v":273.9975,"d":"£274.00"},"Signature date"]
[{"$nulls":4},"RO/TU 80mm/3\"",{"v":306.2325,"d":"£306.23"},"Signature date"]
[{"$nulls":4},"RO/TU 100mm/4\"",{"v":370.7025,"d":"£370.70"},"Signature date"]
[{"$nulls":4},"RO/TU 150mm/6\"",{"v":480.3015,"d":"£480.30"},"Signature date"]
[{"$nulls":4},"RO/TU 200mm/8\"",{"v":664.041,"d":"£664.04"},"Signature date"]
[{"$nulls":4},"RO/TU 250mm/10\"",{"v":1047.6375,"d":"£1,047.64"},"Signature date"]
[{"$nulls":4},"RO/TU > 250mm/10\"","Quoted","Signature date"]
[null,"Housing Installation",null,"MP Diaphragm Meters","U16",{"v":56.36800000000001,"d":"£56.37"},"Signature date"]
[{"$nulls":4},"U25",{"v":56.36800000000001,"d":"£56.37"},"Signature date"]
[{"$nulls":4},"U40",{"v":59.36800000000001,"d":"£59.37"},"Signature date"]
[{"$nulls":4},"U65",{"v":113.73600000000002,"d":"£113.74"},"Signature date"]
[{"$nulls":4},"U100",{"v":113.73600000000002,"d":"£113.74"},"Signature date"]
[{"$nulls":4},"U160",{"v":113.73600000000002,"d":"£113.74"},"Signature date"]
[null,"Housing Installation",null,"LP Rotary/Turbine Meters","RO/TU 50mm/2\"",{"v":118.73600000000002,"d":"£118.74"},"Signature date"]
[{"$nulls":4},"RO/TU 80mm/3\"",{"v":173.10400000000004,"d":"£173.10"},"Signature date"]
[{"$nulls":4},"RO/TU 100mm/4\"",{"v":173.10400000000004,"d":"£173.10"},"Signature date"]
[{"$nulls":4},"RO/TU 150mm/6\"",{"v":173.10400000000004,"d":"£173.10"},"Signature date"]
[{"$nulls":4},"RO/TU 200mm/8\"",{"v":173.10400000000004,"d":"£173.10"},"Signature date"]
[{"$nulls":4},"RO/TU 250mm/10\"",{"v":173.10400000000004,"d":"£173.10"},"Signature date"]
[{"$nulls":4},"RO/TU >250mm/10\"","Quoted","Signature date"]
[null,"Housing Installation",null,"MP Rotary/Turbine Meters","RO/TU 50mm/2\"",{"v":118.73600000000002,"d":"£118.74"},"Signature date"]
[{"$nulls":4},"RO/TU 80mm/3\"",{"v":173.10400000000004,"d":"£173.10"},"Signature date"]
[{"$nulls":4},"RO/TU 100mm/4\"",{"v":173.10400000000004,"d":"£173.10"},"Signature date"]
[{"$nulls":4},"RO/TU 150mm/6\"",{"v":178.10400000000004,"d":"£178.10"},"Signature date"]
[{"$nulls":4},"RO/TU 200mm/8\"",{"v":227.47200000000004,"d":"£227.47"},"Signature date"]
[{"$nulls":4},"RO/TU 250mm/10\"",{"v":227.47200000000004,"d":"£227.47"},"Signature date"]
[{"$nulls":4},"RO/TU >250mm/10\"","Quoted","Signature date"]
["EMS02 Meter Install/Fix","Lifting Gear",null,"MP Diaphragm Meters","U16","Quoted","Signature date"]
[{"$nulls":4},"U25"]
[{"$nulls":4},"U40"]
[{"$nulls":4},"U65"]
[{"$nulls":4},"U100"]
[{"$nulls":4},"U160"]
[null,"Lifting Gear",null,"LP Rotary/Turbine Meters","RO/TU 50mm/2\"","Quoted","Signature date"]
[{"$nulls":4},"RO/TU 80mm/3\""]
[{"$nulls":4},"RO/TU 100mm/4\""]
[{"$nulls":4},"RO/TU 150mm/6\""]
[{"$nulls":4},"RO/TU 200mm/8\""]
[{"$nulls":4},"RO/TU 250mm/10\""]
[{"$nulls":4},"RO/TU >250mm/10\""]
[null,"Lifting Gear",null,"MP Rotary/Turbine Meters","RO/TU 50mm/2\"","Quoted","Signature date"]
[{"$nulls":4},"RO/TU 80mm/3\""]
[{"$nulls":4},"RO/TU 100mm/4\""]
[{"$nulls":4},"RO/TU 150mm/6\""]
[{"$nulls":4},"RO/TU 200mm/8\""]
[{"$nulls":4},"RO/TU 250mm/10\""]
[{"$nulls":4},"RO/TU >250mm/10\""]
[null,"Other",null,"Abortive Call Charge",null,{"v":108.58,"d":"£108.58"},"Signature date"]
[{"$nulls":3},"Quotation (Site Survey)",null,{"v":120,"d":"£120.00"},"Signature date"]

{"sheet":"Table 2","index":1,"n_rows":28,"n_cols":5,"rows_kept":28,"merged":[[20,0,27,0]],"flags":["formulas_cached_only"]}
[]
["Northern Gas Networks Limited"]
["Gas Meter Services Contract"]
["Meterwork Contract Rates"]
[]
["Table 2"]
[]
["Network Services (E&I Work)",null,null," "]
["TMS Job Code","Standard Job","Description","Unit Price","Effective Date"]
["NGM030","N/A","INSTALL / REPLACE CONVERTOR ",{"v":458.79,"d":"£458.79"},"Signature date"]
["NGM031","N/A","AUDIT INSTALLATION (ISSUED AS A STANDALONE JOB)",{"v":194.09,"d":"£194.09"},"Signature date"]
["NGM032","N/A","SITE SURVEY / HAD ASSESSMENT (ISSUED AS A STANDALONE JOB)",{"v":194.09,"d":"£194.09"},"Signature date"]
["NGM034","N/A","MAINTAIN CONVERTOR (PLANNED)",{"v":152.24,"d":"£152.24"},"Signature date"]
["NGM035","N/A","DISCONNECTION OR RECONNECTION OF CONVERTOR (ISSUED AS A STANDALONE JOB)",{"v":134.37,"d":"£134.37"},"Signature date"]
["NGM037","N/A","DISCONNECTION OR RECONNECTION OF C'BOX",{"v":119.44,"d":"£119.44"},"Signature date"]
["NGM039","N/A","REPLACE  CHATTERBOX",{"v":145.26,"d":"£145.26"},"Signature date"]
["NGM041","N/A","REMOVE, CONVERTOR/C'BOX, LF LEAD - EQUIPMENT NO LONGER REQUIRED ON SITE (WHEN ISSUED AS A STANDALONE JOB)",{"v":194.09,"d":"£194.09"},"Signature date"]
["NGM042","N/A","FLOW COMPUTER MAINTENANCE",{"v":656.91,"d":"£656.91"},"Signature date"]
["NGM044","N/A","INVESTIGATE FAULT REPORT / CHECK EQUIPMENT WORKING CORRECTLY AND REPAIR AS NECESSARY",{"v":152.24,"d":"£152.24"},"Signature date"]
["NGM045","N/A","COMMISSION CONVERTOR (WHICH HAS BEEN SUPPLIED AS PART OF THE PRE FABRICATED METER RIG)",{"v":179.16,"d":"£179.16"},"Signature date"]
["EMS04","MPU02","Provide a pulsed output to customer by fitting a 4 port isolation barrier to Meter Installation where Converter is already present. Pulse to be made available to customer via the installation of a junction box.",{"v":174.50398665000003,"d":"£174.50"},"2006-06-01"]
[null,"MPU03","Provide an accessible pulse to customer via the installation of a junction box on a meter installation where datalogger and 4 port isolation barrier is already present.",{"v":111.04902364500002,"d":"£111.05"},"2006-06-01"]
[null,"MPU04","Replace 2 port islation barrier with a 4 port isolation barrier and provide and provide an accessible pulse to customer via the installation of a junction box. ",{"v":142.78218192000003,"d":"£142.78"},"2006-06-01"]
[null,"MPU05","Adjust wiring configuration of existing 4 port isolation barrier and provide an accessible pulse to customer via the installation of a junction box. ",{"v":111.04902364500002,"d":"£111.05"},"2006-06-01"]
[null,"MPU06","Provide a pulsed output to customer by fitting a 4 port isolation barrier to Meter only Installation. Pulse to be made available to customer via the installation of a junction box.",{"v":174.50398665000003,"d":"£174.50"},"2006-06-01"]
[null,"MPU08","Connection Inspection Charge - a Transco provided inspection of the Company's pulse connection where a \"Connection Certificate\" has not been provided to National Grid Metering",{"v":126.90992601000002,"d":"£126.91"},"2006-06-01"]
[null,"MPU09","Disconnection OR Reconnection of Meter Pulse Utilisation equipment (eg to facilitate meter exchnage)",{"v":63.45496300500001,"d":"£63.45"},"2006-06-01"]
[null,"MPU10","Disconnect and remove Meter Pulse Utilisation equipment from site (Equipment no longer required)",{"v":63.45496300500001,"d":"£63.45"},"2006-06-01"]

{"sheet":"Table 3","index":2,"n_rows":45,"n_cols":7,"rows_kept":45,"merged":[[9,0,14,0],[9,1,14,1],[9,2,14,2],[9,3,14,3],[15,0,40,0],[15,1,20,1],[15,2,20,2],[15,3,20,3],[21,1,40,1],[21,2,26,2],[21,3,26,3],[27,2,33,2],[27,3,33,3],[34,2,40,2],[34,3,40,3]],"flags":["formulas_cached_only"]}
[]
["Northern Gas Networks Limited"]
["Gas Meter Services Contract"]
["Meterwork Contract Rates"]
[]
["Table 3"]
[]
["Emergency services (Meter Exchange)",{"$nulls":4}," "]
["Activity Job Code","Notes","NGM Job Ref Type","Description",null,"Unit Price","Effective Date"]
["EMS07a Exchange (Policy)","Abortive calls/No accesses are included in these rates and cannot be charged for separately. Also includes purging and reconnection to consumers pipework.",2600000000,"LP Diaphragm Meters","U16",{"v":55.84,"d":"£55.84"},"2006-06-01"]
[{"$nulls":4},"U25",{"v":59.39,"d":"£59.39"},"2006-06-01"]
[{"$nulls":4},"U40",{"v":111.45,"d":"£111.45"},"2006-06-01"]
[{"$nulls":4},"U65",{"v":111.46,"d":"£111.46"},"2006-06-01"]
[{"$nulls":4},"U100",{"v":135.66,"d":"£135.66"},"2006-06-01"]
[{"$nulls":4},"U160",{"v":135.66,"d":"£135.66"},"2006-06-01"]
["EMS07c Exchange OFMAT","Abortive calls/No accesses are included in these rates and cannot be charged separately. Also includes purging and reconnection to consumers pipework.",2200000000,"LP Diaphragm Meters","U16",{"v":56.67,"d":"£56.67"},"2006-06-01"]
[{"$nulls":4},"U25",{"v":59.4,"d":"£59.40"},"2006-06-01"]
[{"$nulls":4},"U40",{"v":111.46,"d":"£111.46"},"2006-06-01"]
[{"$nulls":4},"U65",{"v":111.46,"d":"£111.46"},"2006-06-01"]
[{"$nulls":4},"U100",{"v":135.69,"d":"£135.69"},"2006-06-01"]
[{"$nulls":4},"U160",{"v":135.69,"d":"£135.69"},"2006-06-01"]
[null,"Genuine abortive visits and third party cancellation charges can be recovered separately and are NOT to be  included in these rates.",2400000000,"MP Diaphragm Meters","U16",{"v":179.59,"d":"£179.59"},"Signature date"]
[{"$nulls":4},"U25",{"v":187.27,"d":"£187.27"},"Signature date"]
[{"$nulls":4},"U40",{"v":322.97,"d":"£322.97"},"Signature date"]
[{"$nulls":4},"U65",{"v":559.96,"d":"£559.96"},"Signature date"]
[{"$nulls":4},"U100",{"v":604.2,"d":"£604.20"},"Signature date"]
[{"$nulls":4},"U160",{"v":628.89,"d":"£628.89"},"Signature date"]
[null,null,2400000000,"LP Rotary/Turbine Meters","RO/TU 50mm/2\"",{"v":423.24,"d":"£423.24"},"Signature date"]
[{"$nulls":4},"RO/TU 80mm/3\"",{"v":472.61,"d":"£472.61"},"Signature date"]
[{"$nulls":4},"RO/TU 100mm/4\"",{"v":690.28,"d":"£690.28"},"Signature date"]
[{"$nulls":4},"RO/TU 150mm/6\"",{"v":949.78,"d":"£949.78"},"Signature date"]
[{"$nulls":4},"RO/TU 200mm/8\"",{"v":1122.67,"d":"£1,122.67"},"Signature date"]
[{"$nulls":4},"RO/TU 250mm/10\"",{"v":1320.15,"d":"£1,320.15"},"Signature date"]
[{"$nulls":4},"RO/TU >250mm 10\"","Quoted","Signature date"]
[null,null,2400000000,"MP Rotary/Turbine Meters","RO/TU 50mm/2\"",{"v":472.61,"d":"£472.61"},"Signature date"]
[{"$nulls":4},"RO/TU 80mm/3\"",{"v":566.86,"d":"£566.86"},"Signature date"]
[{"$nulls":4},"RO/TU 100mm/4\"",{"v":690.28,"d":"£690.28"},"Signature date"]
[{"$nulls":4},"RO/TU 150mm/6\"",{"v":949.78,"d":"£949.78"},"Signature date"]
[{"$nulls":4},"RO/TU 200mm/8\"",{"v":1122.67,"d":"£1,122.67"},"Signature date"]
[{"$nulls":4},"RO/TU 250mm/10\"",{"v":1320.15,"d":"£1,320.15"},"Signature date"]
[{"$nulls":4},"RO/TU > 250mm/10\"","Quoted","Signature date"]
[]
["* See table 1 for lifting gear and other rates"]
[]
[null," "]

{"sheet":"Table 4","index":3,"n_rows":37,"n_cols":7,"rows_kept":37,"merged":[[9,0,34,0],[9,1,14,1],[9,2,14,2],[9,3,14,3],[15,1,34,1],[15,2,20,2],[15,3,20,3],[15,5,20,5],[15,6,20,6],[21,2,27,2],[21,3,27,3],[21,5,27,5],[21,6,27,6],[28,2,34,2],[28,3,34,3],[28,5,34,5],[28,6,34,6]],"flags":["formulas_cached_only"]}
[]
["Northern Gas Networks Limited"]
["Gas Meter Services Contract"]
["Meterwork Contract Rates"]
[]
["Table 4"]
[]
["Emergency services (Meter Exchange)",{"$nulls":4}," "]
["Activity Job Code","Notes","NGM Job Ref Type","Description",null,"Unit Price","Effective Date"]
["EMS08 Exchange (change in load)","Abortive calls/No accesses are included in these rates. ",2200000000,"LP Diaphragm Meters","U16",{"v":55.84,"d":"£55.84"},"2006-06-01"]
[{"$nulls":4},"U25",{"v":59.39,"d":"£59.39"},"2006-06-01"]
[{"$nulls":4},"U40",{"v":111.45,"d":"£111.45"},"2006-06-01"]
[{"$nulls":4},"U65",{"v":111.46,"d":"£111.46"},"2006-06-01"]
[{"$nulls":4},"U100",{"v":135.66,"d":"£135.66"},"2006-06-01"]
[{"$nulls":4},"U160",{"v":135.66,"d":"£135.66"},"2006-06-01"]
[null,"Genuine abortive visits and third party cancellation charges can be recovered separately and are NOT to be  included in these rates.",2400000000,"MP Diaphragm Meters","U16","Quoted","Signature date"]
[{"$nulls":4},"U25"]
[{"$nulls":4},"U40"]
[{"$nulls":4},"U65"]
[{"$nulls":4},"U100"]
[{"$nulls":4},"U160"]
[null,null,2400000000,"LP Rotary/Turbine Meters","RO/TU 50mm/2\"","Quoted","Signature date"]
[{"$nulls":4},"RO/TU 80mm/3\""]
[{"$nulls":4},"RO/TU 100mm/4\""]
[{"$nulls":4},"RO/TU 150mm/6\""]
[{"$nulls":4},"RO/TU 200mm/8\""]
[{"$nulls":4},"RO/TU 250mm/10\""]
[{"$nulls":4},"RO/TU >250mm 10\""]
[null,null,2400000000,"MP Rotary/Turbine Meters","RO/TU 50mm/2\"","Quoted","Signature date"]
[{"$nulls":4},"RO/TU 80mm/3\""]
[{"$nulls":4},"RO/TU 100mm/4\""]
[{"$nulls":4},"RO/TU 150mm/6\""]
[{"$nulls":4},"RO/TU 200mm/8\""]
[{"$nulls":4},"RO/TU 250mm/10\""]
[{"$nulls":4},"RO/TU > 250mm/10\""]
[]
["* See table 1 for lifting gear and other rates"]

{"sheet":"Table 5","index":4,"n_rows":37,"n_cols":7,"rows_kept":37,"merged":[[9,0,34,0],[9,1,14,1],[9,2,14,2],[9,3,14,3],[15,1,34,1],[15,2,20,2],[15,3,20,3],[21,2,27,2],[21,3,27,3],[28,2,34,2],[28,3,34,3]],"flags":["formulas_cached_only"]}
[]
["Northern Gas Networks Limited"]
["Gas Meter Services Contract"]
["Meterwork Contract Rates"]
[]
["Table 5"]
[]
["Emergency services (Meter Removal)",{"$nulls":4}," "]
["Activity Job Code","Notes","NGM Job Ref Type","Description",null,"Unit Price","Effective Date"]
["EMS09 (Meter Removal excluding purging costs). ","These rates include Abortive calls/No accesses. Additional purging cost can be charged on a Time and Material basis.",2200000000,"LP Diaphragm Meters","U16",{"v":55.7,"d":"£55.70"},"2006-06-01"]
[{"$nulls":4},"U25",{"v":55.7,"d":"£55.70"},"2006-06-01"]
[{"$nulls":4},"U40",{"v":81.76,"d":"£81.76"},"2006-06-01"]
[{"$nulls":4},"U65",{"v":81.76,"d":"£81.76"},"2006-06-01"]
[{"$nulls":4},"U100",{"v":103.58,"d":"£103.58"},"2006-06-01"]
[{"$nulls":4},"U160",{"v":103.58,"d":"£103.58"},"2006-06-01"]
[null,"Genuine abortive visits and third party cancellation charges can be recovered separately and are NOT to be  included in these rates.",2400000000,"MP Diaphragm Meters","U16",{"v":169.68,"d":"£169.68"},"Signature date"]
[{"$nulls":4},"U25",{"v":179.55,"d":"£179.55"},"Signature date"]
[{"$nulls":4},"U40",{"v":298.86,"d":"£298.86"},"Signature date"]
[{"$nulls":4},"U65",{"v":445.13,"d":"£445.13"},"Signature date"]
[{"$nulls":4},"U100",{"v":445.13,"d":"£445.13"},"Signature date"]
[{"$nulls":4},"U160",{"v":529.18,"d":"£529.18"},"Signature date"]
[null,null,2400000000,"LP Rotary/Turbine Meters","RO/TU 50mm/2\"",{"v":303.29,"d":"£303.29"},"Signature date"]
[{"$nulls":4},"RO/TU 80mm/3\"",{"v":313.29,"d":"£313.29"},"Signature date"]
[{"$nulls":4},"RO/TU 100mm/4\"",{"v":471.91,"d":"£471.91"},"Signature date"]
[{"$nulls":4},"RO/TU 150mm/6\"",{"v":613.88,"d":"£613.88"},"Signature date"]
[{"$nulls":4},"RO/TU 200mm/8\"",{"v":752.61,"d":"£752.61"},"Signature date"]
[{"$nulls":4},"RO/TU 250mm/10\"",{"v":932.48,"d":"£932.48"},"Signature date"]
[{"$nulls":4},"RO/TU >250mm 10\"","Quoted","Signature date"]
[null,null,2400000000,"MP Rotary/Turbine Meters","RO/TU 50mm/2\"",{"v":323.86,"d":"£323.86"},"Signature date"]
[{"$nulls":4},"RO/TU 80mm/3\"",{"v":370.88,"d":"£370.88"},"Signature date"]
[{"$nulls":4},"RO/TU 100mm/4\"",{"v":690.31,"d":"£690.31"},"Signature date"]
[{"$nulls":4},"RO/TU 150mm/6\"",{"v":922.79,"d":"£922.79"},"Signature date"]
[{"$nulls":4},"RO/TU 200mm/8\"",{"v":1061.52,"d":"£1,061.52"},"Signature date"]
[{"$nulls":4},"RO/TU 250mm/10\"",{"v":1298.99,"d":"£1,298.99"},"Signature date"]
[{"$nulls":4},"RO/TU > 250mm/10\"","Quoted","Signature date"]
[]
["* See table 1 for lifting gear and other rates"]

{"sheet":"Table 6a","index":5,"n_rows":29,"n_cols":7,"rows_kept":29,"merged":[[10,0,28,0],[10,1,28,1],[10,2,15,2],[10,3,15,3],[10,5,15,5],[10,6,15,6],[16,2,21,2],[16,3,21,3],[16,5,21,5],[16,6,21,6],[22,2,28,2],[22,3,28,3],[22,5,28,5],[22,6,28,6]],"flags":["formulas_cached_only"]}
[]
["Northern Gas Networks Limited"]
["Gas Meter Services Contract"]
["Meterwork Contract Rates"]
[]
["Table 6a"]
[]
["Emergency Services (Attend fault and Repair)"]
[{"$nulls":5}," "]
["Activity Job Code","Notes","NGM Job Ref Type","Description",null,"Unit Price","Effective Date"]
["EMS13 Maintenance of Metering Systems (Unplanned and Planned)  ","Meter Maintenance Unplanned. Covers Meter Fault Gas On/Off Situations","UPD8000000/TFM","Repair component and/or exchange faulty Diaphragm Meter. Attend and rectify at first visit wherever possible. ","LP U16","Ad Hoc","Signature date"]
[{"$nulls":4},"LP U25"]
[{"$nulls":4},"LP U40"]
[{"$nulls":4},"LP U65"]
[{"$nulls":4},"LP U100"]
[{"$nulls":4},"LP U160"]
[null,null,"UPD8000000/TFM","Repair component and/or exchange faulty Diaphragm Meter. Attend and rectify at first visit wherever possible. ","MP U16","Ad Hoc","Signature date"]
[{"$nulls":4},"MP U25"]
[{"$nulls":4},"MP U40"]
[{"$nulls":4},"MP U65"]
[{"$nulls":4},"MP U100"]
[{"$nulls":4},"MP U160"]
[null,null,"UPD8000000/TFM","Repair component and/or exchange faulty Rotary/Turbine Meter. Includes initial visit to diagnose fault, restore gas, completion of meter reorder form and subsequent meter exchange, as required by the individual circumstances","LP/MP RO/TU 50mm/2\"","Ad Hoc","Signature date"]
[{"$nulls":4},"LP/MP RO/TU 80mm/3\""]
[{"$nulls":4},"LP/MP RO/TU 100mm/4\""]
[{"$nulls":4},"LP/MP RO/TU 150mm/6\""]
[{"$nulls":4},"LP/MP RO/TU 200mm/8\""]
[{"$nulls":4},"LP/MP RO/TU 250mm/10\""]
[{"$nulls":4},"LP/MP RO/TU >250mm 10\""]

{"sheet":"Table 6b","index":6,"n_rows":145,"n_cols":10,"rows_kept":145,"merged":[[8,0,8,8],[10,0,13,0],[10,7,13,7],[10,8,13,8],[10,9,13,9],[14,0,33,0],[14,7,32,7],[14,8,33,8],[14,9,32,9],[34,0,37,0],[34,7,37,7],[34,8,37,8],[34,9,37,9],[39,0,44,0],[39,7,44,7],[39,8,44,8],[39,9,44,9],[46,0,47,0],[46,7,47,7],[46,8,47,8],[46,9,47,9],[49,0,53,0],[49,7,53,7],[49,8,62,8],[49,9,53,9],[54,0,62,0],[54,7,62,7],[54,9,62,9],[63,0,64,0],[63,7,64,7],[63,8,64,8],[63,9,64,9],[65,0,68,0],[65,7,68,7],[65,8,68,8],[65,9,68,9],[69,0,71,0],[69,7,71,7],[69,8,71,8],[69,9,71,9],[72,0,74,0],[72,7,74,7],[72,8,74,8],[72,9,74,9],[75,0,76,0],[75,7,76,7],[75,8,76,8],[75,9,76,9],[77,0,79,0],[77,7,79,7],[77,8,78,8],[77,9,79,9],[81,0,83,0],[81,7,83,7],[81,8,83,8],[81,9,83,9],[86,0,87,0],[86,7,87,7],[86,8,87,8],[86,9,87,9],[104,0,105,0],[104,7,105,7],[104,9,105,9],[108,0,111,0],[108,8,111,8],[112,0,115,0],[112,8,114,8]],"flags":["formulas_cached_only"]}
[]
["Northern Gas Networks Limited"]
["Gas Meter Services Contract"]
["Meterwork Contract Rates"]
[]
["Table 6b"]
[]
["Network Services (Governor Maintenance Work)"]
["I&C MAINTENANCE CHARGES"]
["TMS Job Code","Standard Job","Description","NW","WM","EE","LO","Unit Cost","Work Description","Effective Date"]
["NGM01","M2101A","Routine Inspection Service Governor",{"$nulls":4},{"v":148.1,"d":"£148.10"},"Planned maintenance inspections of service governors > 75Mbar < 7Bar at frequencies stated in T/PM/MAINT/2 Part 1. Maintenance activities to be completed are listed in Appendix A, B and C of the same document. These apply to category 1 and 2 installations as defined in section 5 of T/PM/MAINT/2 Part 1. This includes any relevant maintenance inspections ES/94/13 Part 6 under T/PM/PS/3 to be performed as part of the PSSR 2000 regulations.This product will include adortive visits due to no access, etc.","Signature date"]
[null,"M2102A","Functional Check Service Governor"]
[null,"P0019A","ES/94/13 Pt6 PPDs Domestic Type Serv Reg"]
[null,"M0001F","Visual insp. AbGnd Service Gov-LTS"]
["NGM02","M2201A","Routine Check <7 bar sites",{"$nulls":4},{"v":271.52,"d":"£271.52"},"Planned maintenance inspections of I&C Governor installations < 7 Bar at frequencies stated in T/PM/MAINT/2 Part 2 Appendix E, F, G, H, J and K. References should also be made to Appendix L, M and N of the same document. This will also include, if applicable to the site, a PSSR integrity inspection as stated and detailed in T/PM/PS/3 - ES/94/13 Part 2.","Signature date"]
[null,"M2202A","Func Check <7 bar -1 stream RCM sites"]
[null,"M2202B","Func Check <7 bar -2 stream RCM sites"]
[null,"M2202C","Func Chk <7b Kiosk-3 stream RCM sites"]
[null,"M2202X","Functional Check <7 bar RCM sites"]
[null,"M2204A","Func Check <7 bar -1 stream Non RCM"]
[null,"M2204B","Func Check <7 bar -2 stream Non RCM"]
[null,"M2204C","Func Chk <7b Kiosk-3 stream Non RCM"]
[null,"M2204X","Functional Check <7 bar - Non RCM"]
[null,"M2216A","Functional Check <7bar -  Filters"]
[null,"M2217A","Funct. Chk- 2-7b Remote opp Crit Vlve"]
[null,"M2217B","Funct. Chk- 2-7b Local opp Crit Valve"]
[null,"P0015A","ES/94/13 Pt2 - PPD's PRS's < 7 Bar RCM"]
[null,"P0015B","ES/94/13 Pt2 < 7 bar -2 stream RCM sites"]
[null,"P0015C","ES/94/13 Pt2 Kiosk-3 stream RCM sites"]
[null,"P0015X","ES/94/13 Pt2 <7 bar RCM sites"]
[null,"P0031A","ES/94/13 Pt2 <7bar -1 str Non RCM"]
[null,"P0031B","ES/94/13 Pt2 <7bar -2 str Non RCM"]
[null,"P0031X","ES/94/13 Pt2 -PPD's PRS's <7bar Non RCM"]
[null,"M0037A","Meter Oil Check",{"$nulls":4},282.91,null,"2006-06-01"]
["NGM03","M2215A M/E","Maj o/haul-Filters<7b-Multi Element /set",{"$nulls":4},"Ad hoc","Major Overhaul of I&C Governor installation < 7 Bar at a 6 Yearly frequency as stated in T/PM/MAINT/2 Part 2 section 7 and Appendix H. Due to the varying size of these sites, the differing costs of spares and the time involved to undertake these tasks the costing will be done on an individual site basis and submitted via the TMS ad hoc process.","Signature date"]
[null,"M2215B S/E","Maj o/haul-Filters<7b-AGI Single Element"]
[null,"M2215C","Maj o/haul-Filters<7b-Min Offtake"]
[null,"M2205A","Major Overhaul <7 bar Press Reduction"]
["NGM04","M0001C","Visual insp.-AbGnd AGI-LTS",{"$nulls":4},{"v":185.13,"d":"£185.13"},"6 yearly above ground maintenance examination of plant no longer subjected to PSSR inspections as per T/PM/MAINT/2 Part 2 section 7.2.4, Appendix C.4. and Appendix J.","Signature date"]
["NGM05","M0002A","CIPS of Bur'd Pipe/wk on AGI-Complex-NTS",{"$nulls":4},{"v":477.75,"d":"£477.75"},"6 yearly maintenance examination of below ground plant no longer subjected to PSSR inspections as per T/PM/MAINT2/ Part 2 Appendix J and T/PL/ECP1. This will include the completion of any relevant documentation","Signature date"]
[null,"M5014A","CP Monitoring Functional check - S/Anode"]
[null,"M5014B","CP Monitoring Functional check - Imp Cur"]
[null,"M5015A","CP Monitoring Interim insp - Imp Cur"]
[null,"M5016A","CP Monitoring Major inspection - S/Anode"]
[null,"M5016B","CP Monitoring Major inspection - Imp Cur"]
["NGM06","M0003A","Maintenance Painting Assessment",{"$nulls":4},{"v":135.76,"d":"£135.76"},"Painting examimations of all the equipmet as per T/PM/MAINT/2 Part 2. Appendix K. This will be on a 6 yearly frequency. ","Signature date"]
["NGM07","M5014A","CP Monitoring Functional check - S/Anode",{"$nulls":4},{"v":149.3,"d":"£149.30"},"Functional checks and major inspections on >75Mbar<7bar PRI SAC CP systems to T/PL/ECP1","Signature date"]
[null,"M5016A","CP Monitoring Major inspection - S/Anode"]
["NGM08","M2301A","Routine Check - A - All systems on site",{"$nulls":4},{"v":74.05,"d":"£74.05"},"Monthly routine check for > 7 Bar sites without remote monitoring facilities as per T/PM/MAINT2/Part 3. Appendix A.","Signature date"]
["NGM09","M2303A","Func Chk-Filters B3-Multi Element /set",{"$nulls":4},{"v":296.21,"d":"£296.21"},"Routine inspections and maintenance activities on > 7 bar sites with or without remote monitoring facilities as per T/PM/MAINT2/Part 3. Appendix A, B, C, D, AND E. This includes inspections required under PSSR 2000 which include:  ES/94/13 Part 1, ES/94/13 Part 5. Water analysis costs will be via ad-hoc billing procedure.","Signature date"]
[null,"M2303B","Func Chk-Filters B3-AGI Single Element"]
[null,"M2304A","Func Chk-B4A-Press Red Equip >7bar -Main"]
[null,"M2305A","Func Chk,B4B Pres Red. Equip(Smal Bore)"]
[null,"M0006X","Indep Diff Filter Chk-Dusty N'wk -U/knwn"]
["NGM09","P0014A","ES/94/13 Pt1 - PPD's PRS's > 7 Bar",{"$nulls":4},{"v":296.21,"d":"£296.21"},null,"Signature date"]
[null,"P0018A","ES/94/13 Pt5 PPD's Small Bore Reg Inst."]
[null,"M2319A","Site Functional Check - B1 General"]
[null,"M2306B","Func.Ch-Mod.Boil&HE-comp Sys-exl wat sam"]
[null,"M2306D","Func.Ch-Mod boiler sys-exl wat sam"]
[null,"M2307A","Func. Chk - WB Heater - incl water sam"]
[null,"M2307B","Func.Ch-Mod boiler sys-inc wat sam"]
[null,"M2307D","Func.Ch-Mod boiler sys-inc wat sam"]
[null,"M2306A","Func. Chk - WB Heater - exl water sam"]
["NGM10","M2311A","Maj o/haul-Filters C2-Multi Element /set",{"$nulls":4},{"v":246.84,"d":"£246.84"},"2 yearly major filter overhaul on > 7 Bar sites as per T/PM/MAINT2/Part 3. Appendix C. Material costs dependant on usage via TMS ad-hoc billing process","Signature date"]
[null,"M2311B","Maj o/haul-Filters C2-AGI Single Element"]
["NGM11","M2312A","Major Overhaul - C3A Press Red. Equip",{"$nulls":4},"Quoted","Major overhaul on > 7 Bar sites as determined by functional check, or sites deemed to require a major overhaul after risk assessment as per Guidance note BS EN ISO 9001: 2000. As per T/PM/MAINT2/Part 3. Appendix C. Due to the varying size of these sites, the differing costs of spares and the time involved to undertake these tasks the costing will be done on an individual site basis and submitted via the TMS ad hoc billing process.","Signature date"]
[null,"M2320A","Major O/Haul small bore regs"]
[null,"M2314A","Major overhaul - C4 WB Heater"]
[null,"M2314B","Major overhaul - C4 Mod.Boil&HE-comp Sys"]
["NGM12","P0025A","ES/94/15 Pt1-HP Filters-Multi Element",{"$nulls":4},{"v":246.84,"d":"£246.84"},"6 yearly filter visual inspections on > 7 Bar sites as per T/PR/PS/3. ES/94/15 Part 1. ","Signature date"]
[null,"P0025C","ES/94/15 Pt1 HP Filters-MO"]
[null,"P0025X","ES/94/15 Pt1-HP Filters-Uknown Elements"]
["NGM13","P0026A","ES/94/15 Pt2 HP Filters-Multi Element",{"$nulls":4},"Ad hoc","12 yearly NDT Filter inspection and remedial painting on > 7 Bar sites as per T/PR/PS/3. ES/94/15 Part 2. Due to the varying size of these sites and the specialist time involved to undertake these tasks the costing will be done on an individual site basis and submitted via the TMS ad hoc billing process.","Signature date"]
[null,"P0026C","ES/94/15 Pt2 HP Filters-MO"]
[null,"P0026X","ES/94/15 P2-HP Filters-Uknown Elements"]
["NGM14","M0004A","Maint Exam's: VS02 Water Bath Heaters",{"$nulls":4},"Ad hoc","10 yearly pre-heater inspection on > 7 bar sites as per T/PM/MAINT2/Part 3. Appendix D. Due to the varying size of these sites, cranage and NDT inspection coupled with the differing costs of spares and the time involved to undertake these tasks the costing will be done on an individual site basis and submitted via the TMS ad hoc billing process.","Signature date"]
[null,"M0005A","Maint Exam's VS02 Shell Tube Heat Exch's"]
["NGM15","M0003A","Maintenance Painting Assessment",{"$nulls":4},{"v":172.29,"d":"£172.29"},"6 yearly VS02 inspections of all above ground pipework including any relevant paint assessment as per T/PM/MAINT 2 Part 3 Appendix D & E. This will include a completion of any relevant documentation. ","Signature date"]
[null,"M0001C","Visual insp.-AbGnd AGI-LTS"]
[null,"P0007A","ES/94/10 Pt1 - Gen. Pressure Vessels A/G"]
["NGM16","M0002A","Maint Exam: Bur'd Pipe/wk & componants",{"$nulls":4},{"v":477.75,"d":"£477.75"},"6 yearly below ground installation pipework inspection, close interval potential survey (CIPS), in accordance with T/PL/ECP 1 as stated in T/PM/MAINT 2/ Part 3 Appendix d. This will include a completion of an relevant documentation. ","Signature date"]
["NGM17","M5014B","CP Monitoring Functional check - Imp Cur",{"$nulls":4},{"v":134.37,"d":"£134.37"},"Monthly, interim and major cathodic protection (CP) inspections of single tranformer rectifier (TR) systems operating on >7bar PRI's to T/PL/ECP1","Signature date"]
[null,"M5015A","CP Monitoring Interim insp - Imp Cur"]
[null,"M5016B","CP Monitoring Major inspection - Imp Cur"]
["NGM18","M5014A","CP Monitoring Functional check - S/Anode",{"$nulls":4},{"v":134.37,"d":"£134.37"},"6 monthly and 2 yearly CP inspections of sacrificial anode current (SAC) systems on >7bar PRI's to T/PL/ECP1","Signature date"]
["NGM19","M0047A","Miscellaneous Site Husbandry",{"$nulls":4},"Ad hoc","Miscellaneous site husbandry activities such as grass cutting, hedge trimming & weedkilling. Due to the varrying size of these sites and differing tasks, the costing will be done on an individual site basis and submitted via the TMS ad hoc billing process.","Signature date"]
["NGM20","M2308A","LTS Funct. Chk- B6A Local opp Crit Valve",{"$nulls":4},{"v":197.47,"d":"£197.47"},"2 monthly/24 monthly operation of all on site critical and non critical valves as stated in T/PM/MAINT2/ Part 3, Appendix B. *This does not include any valves located in confined spaces that require a permit to work & method statement.","Signature date"]
[null,"M2309A","LTS Funct. Chk- B6B Loc opp NonCrit Valve"]
["TMS030","N/A","INSTALL / REPLACE CONVERTOR",{"$nulls":4},"To follow","Work instruction received from TM, logged on local database and issued to technician. If new installation a site survey is required to check for suitable connections to the rig etc. Materials ordered/obtained. Installation date agreed with customer/TM and Network Services Team as required.Travel to site, obtain access, keys, induction training.Risk assessment, site survey, gas free check, ventilate building. Install pipework, valves, cabling, ducting and converter. Take meter reads and set converter to match.Allow time for meter movement and re check meter and converter reads. Ring datalogging if a logger is present.Note converter and meter details, make, manufacturer, serial number etc. Ring TM with details. Return completed paperwork to office where a new site file and database record is set up. Completed paperwork sent to TM. Invoice raised. Return to site in approx. two weeks to audit installation to ensure corrector is working correctly."]
["TMS031","N/A","AUDIT INSTALLATION",{"$nulls":4},"To follow","Audit installation to ensure corrector is working correctly.Process audit sheets"]
["TMS032","N/A","SITE SURVEY / HAD FORM",{"$nulls":4},"To follow","Site surveys are required to check for suitable connections to the rig for converters and to the meter /converter for EMS and Chatterbox installations. Also the site zoning and ventilation needs to be checked to comply with DESEAR and ATEX reg’s."]
["TMS033","N/A","INSTALL DATALOGGER",{"$nulls":4},"To follow","Work instruction received from TM, logged on local database and issued to technician. If new installation a site survey is required to check for BT and LF connections to the rig etc. Materials ordered/obtained. Installation date agreed with customer/TM and Network Services Team as required.Travel to site, obtain access, keys, induction training.Risk assessment, site survey, gas free check, ventilate building. Install cabling, ducting and datalogger. Take meter reads and inform datalogging. Note datalogger and meter details, make, manufacturer, serial number etc. Ring datalogging with details. Return completed paperwork to office where a new site file and database record is set up. Completed paperwork sent to TM. Invoice raised. "]
["TMS034","N/A","MAINTAIN CONVERTOR",{"$nulls":4},"To follow","From local data base (e.g. Quickwin) print work order and issue to technician. Travel to site, obtain access, keys, induction training. Risk assessment, site survey, gas free check, ventilate building. Visual check of pipework, wiring, ducting etc. Take initial reads of meter and converter. Converter calibration will depend on make and model. Calibrate temperature, pressure and flow using Druck, temperature probe and multimeter etc. Take final set of reads and compare with previous records to ensure correct operation of converter. Return completed paperwork to office where local database and office files are updated. Completed paperwork sent to TM. Invoice raised. "]
["TMS035","N/A","DISCONNECTION / RECONNECTION CONVERTOR",{"$nulls":4},"To follow","Disconnect is due to fault on meter or putting the convertor on by pass. Reconnect should be booked with TMS034"]
["TMS036","N/A","DISCONNECTION / RECONNECTION DATALOGGER",{"$nulls":4},"To follow","Similar to Install Datalogger for reconnection. For Disconnection the reverse of installation with all equipment removed."]
["TMS037","N/A","DISCONNECTION / RECONNECTION C'BOX",{"$nulls":4},"To follow","Disconnect C/Bax, LF Lead etc"]
["TMS038","N/A","FIT CHATTERBOX",{"$nulls":4},"To follow","Work instruction received from TM, logged on local database and issued to technician. If new installation a site survey may be required to check for suitable connections to the meter/Converter. Materials ordered/obtained. Installation date agreed with customer/TM and Network Services Team as required.Travel to site, obtain access, keys, induction training.Risk assessment, site survey, gas free check, ventilate building. Install cabling, ducting and Chatterbox.Meter and converter reads taken before and after installing Chatterbox ensure correct operation of the system. Datalogging/TM informed as required.Return completed paperwork to office where office files and database records are updated. Completed paperwork sent to TM. Invoice raised. "]
["TMS039","N/A","UPGRADE CHATTERBOX",{"$nulls":4},"To follow","Upgrade 2 port opt-isolator to 4-port & provide access to meter pulse port. Adjust"]
["TMS040","N/A","FIT EMS",{"$nulls":4},"To follow","Work instruction received from TM, logged on local database and issued to technician. If new installation a site survey may be required to check for suitable connections to the meter/Converter. Materials ordered/obtained. Installation date agreed with customer/TM and Network Services Team as required.Travel to site, obtain access, keys, induction training.Risk assessment, site survey, gas free check, ventilate building. Install cabling, ducting and Chatterbox.Meter and converter reads taken before and after installing Chatterbox ensure correct operation of the system. Datalogging/TM informed as required.Return completed paperwork to office where office files and database records are updated. Completed paperwork sent to TM. Invoice raised. "]
["TMS041","N/A","REMOVE, CONVERTOR/C'BOX, LF LEAD",{"$nulls":4},"To follow","Remove all quipment from site, remove maintenance information from Database."]
["TMS042","N/A","FLOW COMPUTER MAINTENANCE",{"$nulls":4},"To follow","Take down all asset detailsCalibrate Pressure transmitterZero/intermediate and full scaleCalibrate Temp TransmitterCalibrate inputs to flow computerStart readings/ End readingsInput frequency for meter run testResynch readings with TMS"]
["TMS043","N/A","ABORTIVE CALL",{"$nulls":4},"To follow","Cannot complete work, inform end user, fill in near miss, replan work."]
["TMS044","N/A","ATTEND TO FAULT",{"$nulls":4},"To follow","Attend to fault,(inc request authorisation to repair/ replace). This job should not be booked as an addition to any other job."]
["TMS045","N/A","COMMISSION CONVERTOR",{"$nulls":4},"To follow","Commission convertor, when corrector has been delivered pre installed on a meter rig."]
["NGM050","N/A","MAINT 11 3 MONTHLY RCD CHECK",{"$nulls":4},{"v":104.51,"d":"£104.51"},"Confirm model, make, type, B.S ref R.C.D.Carry out functional testRecord all findings electronically","Signature date"]
[null,"E1144A","MAINT 11 RCD MECHANICAL TRIP (ELEC)"]
["NGM051","N/A","MAINT 11 INTERMEDIATE MAINT (ANNUAL)",{"$nulls":4},{"v":373.24,"d":"£373.24"},"Above R.C.D. checks, in addition to:Full visual check of electrical and earthing installation for damage, deterioration etc;Check identification of cables and equipmentRecord all findings electronically","Signature date"]
["NGM052","E0001A","MAINT 11 FULL MAINT",{"$nulls":4},"Site Specific ","Dismantle all electrical fittings;Measure all cable resistances;Check all cables, glands and junctions;Validify electrical drawings (including correct location of equipment within zones)Record all findings electronically.","Signature date"]
["NGM055","N/A","12 MONTHLY MAINT (MAINT 12) - Convertor only site",{"$nulls":4},{"v":298.6,"d":"£298.60"},"This is an annual intermediate instrumentation maintenance.This involves a spot check on each analogue and a re-calibration on any ‘inaccurate’ instruments. This maintenance also requires the technician to confirm the change of state of every digital alarm, but not necessarily its set point, thus covering all input/output functionality on site.The asset register will also be updated on this site visit.","Signature date"]
[null,"N/A","12 MONTHLY MAINT (MAINT 12) - Flow Computer Site",{"$nulls":4},567.33,null,"Signature date"]
[null,"N/A","12 MONTHLY MAINT (MAINT 12) - Complex sites",{"$nulls":4},806.21,null,"Signature date"]
[null,"N/A","12 MONTHLY MAINT (MAINT 12) - BP Saltend",{"$nulls":4},2478.34,null,"Signature date"]
["NGM056","N/A","24 MONTHLY MAINT (MAINT 12) - Convertor only site",{"$nulls":4},{"v":298.6,"d":"£298.60"},"This is a bi-annual instrumentation maintenance (per meter stream).This would involve a full (zero, intermediate range and full range) check of each instrument.All digitals would be checked, including the switching points and hysteresis.Additionally, a TMM10 maintenance and inspection would be carried out.The asset detail register would again be updated.Other on site checks would include:Charger test;Battery discharge test;Controls (heating/valves/ E/P)Inspect metering equipment (turbines/orifice plates)Prove functionality of isagraph software.","Signature date"]
[null,"N/A","24 MONTHLY MAINT (MAINT 12) - Flow computer site",{"$nulls":4},686.77,null,"Signature date"]
[null,"N/A","24 MONTHLY MAINT (MAINT 12) - Complex sites",{"$nulls":4},1045.08,null,"Signature date"]
[null,"N/A","24 MONTHLY MAINT (MAINT 12) - BP Saltend",{"$nulls":4},{"v":4867.1,"d":"4867.10"},null,"Signature date"]
["EMS13 cont.","NS04a","install/exchange Datalogger",{"$nulls":6},"Signature date"]
[null,"NS04b","install/exchange Datalogger + corrector"]
[null,"NS04c","Install/exchange Corrector"]
[null,"NS04d","Remove Datalogger"]
[null,"NS04e","Remove Datalogger + corrector"]
[null,"NS04e","Remove Corrector"]
[null,"NS07d","Discon and recon of remote metering equipment"]
[null,"NS13f","DM and NDM Logger maint and fault repairs"]
[null,"NS13g","Corrector maintentance and fault repairs"]
[null,"Meter Maintenance","LP/MP Rotory/Turbine"]
[{"$nulls":8},"Maintain Datalogger"]
[{"$nulls":8},"CRDS Check  Reads"]
{"$rows_empty":16}
[null,null,"  "]